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A Vessel Monitoring Plan (VMP) is a document prepared by the Concession Holder and their chosen electronic monitoring (e‑monitoring) service provider that describes the vessel’s e‑monitoring system, including its equipment specifications, installation and configuration, and demonstrates how the system records the fishing activities required for the relevant fishery.
The purpose of the VMP is to enable AFMA to confirm that a type‑approved e‑monitoring system is used and that it has been installed and configured to meet AFMA’s fishery‑specific requirements (refer to Annex 1).
If AFMA determines that the installation or configuration of the e‑monitoring system has not met AFMA’s requirements, the Concession Holder may be required to take corrective action. This may include revising the VMP, adjusting the installation or configuration of the e‑monitoring system, and providing an updated VMP form to AFMA. AFMA may also require additional information to demonstrate that any identified issues have been addressed before the e-monitoring system is considered suitable for ongoing use.





[bookmark: _Toc244265473]Section 1. Concession Holder and Vessel Information (Concession holder must complete Section 1 before submitting to AFMA)
1.1 Concession Holder 
	Business Name
	

	Full Name
	

	Phone
	

	Mobile
	

	Email
	



1.2 Vessel Details
	Vessel Name
	

	Vessel Call Sign
	

	International Maritime Organisation (IMO) number
	

	Homeport
	

	Vessel Length Overall (LOA)
	

	Gross Tonnage
	

	Target Fishery
	

	Fishing Method Used
	





[bookmark: _Toc244265474]Section 2. E-monitoring System Installation 
(E-monitoring service provider representative and/or the Concession Holder are to complete Section 2 before submitting to AFMA)
E-monitoring Service Provider Details
	E-monitoring Service Provider Business 
	

	Services Provided
	

	Office Location
	

	Phone
	

	Email
	


Camera Installation Overview 
The installed camera positions and their range of views are as displayed on the vessel image below. 
IMPORTANT NOTE: The number and position of cameras installed on the vessel MUST cover areas, actions and minimum data requirements outlined in the Fishery Specific Requirements (refer to Annex 1).
The below camera position and range of view diagram is an example for a trawl vessel as guidance. Please insert the vessel specific outlay of each camera installed on a vessel within a diagram below. If required, AFMA can provide a diagram template upon request.


.


	
[image: A diagram of a boat
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Comments: 



















Camera specifications and range of view are displayed below. 
	[bookmark: _Hlk209426649]Camera No. 
	C1
	Camera Install Location

	Area Covered 
(Refer to Fishery Specific Requirements in Annex 1) 
	
	Insert Image

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear. 

	Action Covered
(Refer to Fishery Specific Requirements in Annex 1)
	
	

	Minimum Data Requirement Recorded
(Refer to Fishery Specific Requirements in Annex 1)
	
	

	Camera Make and Model 
	
	

	Frame Per Second 
	
	

	Resolution
	
	Camera View

	Trigger Settings
	
	Insert Image

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear. 

	Recording Exceptions
	
	

	Run on Time
	
	

	Weather Resistance
	
	



	Camera No. 
	C2
	Camera Install Location

	Area Covered
(Refer to Fishery Specific Requirements in Annex 1)
	
	Insert Image

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear. 

	Action Covered
(Refer to Fishery Specific Requirements in Annex 1)
	
	

	Minimum Data Requirement Recorded
(Refer to Fishery Specific Requirements in Annex 1)
	
	

	Camera Make and Model 
	
	

	Frame Per Second 
	
	

	Resolution
	
	Camera View

	Trigger Settings
	
	Insert Image

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear. 

	Recording Exceptions
	
	

	Run on Time
	
	

	Weather Resistance
	
	



	Camera No. 
	C3
	Camera Install Location

	Area Covered
(Refer to Fishery Specific Requirements in Annex 1)
	
	Insert Image

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear. 

	Action Covered
(Refer to Fishery Specific Requirements in Annex 1)
	
	

	Minimum Data Requirement Recorded
(Refer to Fishery Specific Requirements in Annex 1)
	
	

	Camera Make and Model 
	
	

	Frame Per Second 
	
	

	Resolution
	
	Camera View

	Trigger Settings
	
	Insert Image

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear. 

	Recording Exceptions
	
	

	Run on Time
	
	

	Weather Resistance
	
	



	Camera No. 
	C4
	Camera Install Location

	Area Covered
(Refer to Fishery Specific Requirements in Annex 1)
	
	Insert Image

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear. 

	Action Covered
(Refer to Fishery Specific Requirements in Annex 1)
	
	

	Minimum Data Requirement Recorded
(Refer to Fishery Specific Requirements in Annex 1)
	
	

	Camera Make and Model 
	
	

	Frame Per Second 
	
	

	Resolution
	
	Camera View

	Trigger Settings
	
	Insert Image

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear. 

	Recording Exceptions
	
	

	Run on Time
	
	

	Weather Resistance
	
	



	Camera No. 
	C5
	Camera Install Location

	Area Covered
(Refer to Fishery Specific Requirements in Annex 1)
	
	Insert Image

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear. 

	Action Covered
(Refer to Fishery Specific Requirements in Annex 1)
	
	

	Minimum Data Requirement Recorded
(Refer to Fishery Specific Requirements in Annex 1)
	
	

	Camera Make and Model 
	
	

	Frame Per Second 
	
	

	Resolution
	
	Camera View

	Trigger Settings
	
	Insert Image

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear. 

	Recording Exceptions
	
	

	Run on Time
	
	

	Weather Resistance
	
	



Have the cameras been positioned to allow crew to safely clean while the vessel is at sea?
            Yes             No       (Tick one box)

Have the cameras been positioned to minimise the accumulation of sea salt or water drops on the lens? 
            Yes             No       (Tick one box)

Have the cameras been positioned to minimise the effects from glare from deck lights at night and/or reflected light? 
            Yes             No       (Tick one box)

Have the cameras been positioned to minimise obstruction of the camera’s view by gear or crew during fishing activities?
            Yes             No       (Tick one box)

Installation of Other System Components 
The following system parts below have been installed on the vessel. 
Add or remove installed items as applicable. 

	Installed Item
	Location
	Specification
	Details

	Control Centre
	Insert Image of installed Item

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear.
	Install location
	

	
	
	Manufacturer
	

	
	
	Make and model
	

	
	
	Function
	

	
	
	Capacity
	

	
	
	Recording time
	

	
	
	Redundant power supply
	

	
	
	Security and protection
	

	
	
	Software version
	

	
	
	Operating system
	

	
	
	Video compression
	

	Satellite Modem


	Insert Image of installed Item

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear.
	Install location
	

	
	
	Function
	

	
	
	Water resistance
	

	GPS
Receiver
	Insert Image of installed Item

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear.
	Install location
	

	
	
	Function
	

	
	
	Records
	

	
	
	Water resistance
	

	POE Switch
	Insert Image of installed Item

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear.
	Install location
	

	
	
	Function
	

	Sensor(s)


	Insert Image of installed Item

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear.
	Install location
	

	
	
	Function
	

	
	
	Units
	

	
	
	Threshold Values
	

	
	
	Data recording frequencies
	

	Monitor

	Insert Image of installed Item

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear.
	Install location
	

	
	
	Function
	

	Keyboard

	Insert Image of installed Item

All personal and commercial sensitive information must be removed from images. This includes, but is not limited to, people’s faces, timestamps, vessel positions, logos, and/or proprietary fishing gear.
	Install location
	

	
	
	Function
	



Radio Frequency Interference
Following installation, the radio frequencies emitted by the e‑monitoring system were tested to determine if they interfered with the vessel’s safety and navigational equipment on ___ /___ /___ at __________.
Has the e-monitoring system shown to be capable of functioning in close physical proximity to other onboard electrical and hydraulic equipment and not impact (e.g. through radio frequency interference) the proper functioning of other onboard safety and navigational equipment on the vessel?
            Yes             No       (Tick one box)

[bookmark: _Toc244265475]Section 3. Installation Declaration (E-monitoring service provider representative and the Concession Holder must complete and sign Section 3 before submitting it to AFMA)
3.1 E-monitoring Service Provider 
On behalf of ______________, I hereby declare that an AFMA type approved e-‑monitoring system was successfully installed on this fishing vessel on ___ /___ /___ at ___________ port location and that all system components are installed and configured in accordance with Section 2 above. 

____________________________________________
Business Name

____________________________________________
Representative Name 

____________________________________________
Signature & Date

3.2 Vessel Representative 
I ____________, hereby declare that the details in Section 1 and 2 of this VMP are true and accurate to the best of my knowledge. 
I understand I may be required to modify e-monitoring system components to enable the collection of minimum data requirements for the fishery.
I understand that any changes to this VMP will need to be communicated and submitted to AFMA immediately or I may be deemed as not compliant with fishing with an operational e-monitoring system.

____________________________________________
Business Name

____________________________________________
Concession Holder Name 

____________________________________________
Signature & Date


FOR AFMA USE ONLY
[bookmark: _Toc244265476]Section 4. Data Completeness (AFMA representative must complete and sign Section 4 to confirm the e-monitoring system has met AFMAs Requirements)
4.1 Encryption & Decryption
Was AFMA able to successfully decrypt e-monitoring information using the decryption keys supplied by the e-monitoring service provider?
            Yes             No       (Tick one box)

Comment:



4.2 Data Review 
Were all e-monitoring records recorded by the system and stored on the external data drive?
             Yes 	      No     (Tick one box)
Comment:



Was AFMA able to ingest and review all e-monitoring records into AFMAs review software? 
             Yes 	      No     (Tick one box)
Comment:
[Insert image(s) of data ingested into Tator for completeness]


Was AFMA able to review the information on the e-monitoring records to collect minimum data requirements for the fishery? 
             Yes 	      No     (Tick one box)
Comment:
[Refer to minimum data requirements in Annex1]


4.3 Near Real Time
Did the e-monitoring system record and transmit all near real time records to AFMA?
             Yes 	      No     (Tick one box)
Comment:




Was near real time information transmitted to AFMA on an hourly basis while the vessel was out at sea?
            Yes 	      No     (Tick one box) 

Comment:
[Insert image of near real time records ingested into the AFMA database and/or trackwell]


4.4 Modifications
Are modifications required? 	
            Yes 	      No     (Tick one box)
If yes, modifications include: 


4.5 Australian Fisheries Management Authority 

I ___________, have undertaken a data completeness testing and believe that the type-approved e-monitoring system has been installed and configured to meet AFMAs Fishery Specific Requirements for the North West Slope Trawl Fishery and Western Deepwater Trawl Fishery E-monitoring Program. 

____________________________________________
AFMA Representative Name

____________________________________________
Position Title 

____________________________________________
Signature & Date

[bookmark: _Toc244265477]Annex 1. Fishery Specific Requirements for the North West Slope Tawl and Western Deepwater Trawl Fisheries
AFMA type-approved e-monitoring systems used in the North West Slope Trawl Fishery and the Western Deepwater Trawl Fishery (known collectively as the Western Trawl Fisheries) must use cameras to record the occurrence of fishing events, all catch interactions, including interactions with ETP species, and the use of mitigation device(s). 
The e-monitoring system cameras must be configured to cover and collect the following areas, actions and minimum data requirements on Western Trawl Fisheries vessels:
Areas Covered
Areas that cameras are required to cover include: 
· area where the trawl gear is set and hauled, 
· hopper where the catch is spilled from the nets,
· conveyor where the catch is sorted, and 
· processing area where the catch is stored.
Actions Covered
Actions that cameras are required to cover include:
· deployment and retrieval of fishing gear, 
· all netted catch species (both retained and discarded), 
· the fate and life status of bycatch byproduct species of interest, and 
· any interactions with ETP species.
Minimum Data Requirements 
Within these areas and actions covered, the minimum data requirements to be collected on prawn trawl vessels are outlined in Table 1.
Table 1. General areas/activities monitored by onboard cameras to meet minimum data requirements for Western Trawl Fisheries vessels.
	Area Covered
	Action Covered
	Minimum data requirements to be captured for video review

	Stern
	ETP species interactions and drop-outs when cod-ends lifted from water 
	Position, date, and time

	
	
	Species (lowest taxonomic group)

	
	
	Number

	
	
	Fate 

	
	
	Life status

	
	Hauling operation
	Start/end position, date, and time

	Sorting conveyor
	ETP species interactions during sort, opportunity for close-up species identification
	Position, date, and time

	
	
	Species (lowest taxonomic group)

	
	
	Number

	
	
	Fate 

	
	
	Life status

	Hopper
	ETP species interactions in spill
	Position, date, and time

	
	
	Species (lowest taxonomic group)

	
	
	Number

	
	
	Fate 

	
	
	Life status

	Processing area
	Retention of species of interest
	Position, date, and time

	
	
	Species (lowest taxonomic group)

	
	
	Number

	
	
	Fate 

	
	
	Life status



On most Western Trawl Fisheries vessels, an aft facing camera is positioned to record the setting and hauling of the gear, interactions in the throat of the net, and dropouts when the cod-end is lifted from the water, a second camera is positioned over the hopper to record ETP species interactions when the nets are spilled, a third camera is positioned directly over the conveyor to identify ETP species during the sort, and a fourth camera is positioned to record the processing area where the catch is stored. An example of possible camera placement(s) to meet minimum data requirements for Western Trawl Fisheries vessels is shown in Figure 1 for guidance.
Figure 1. E-monitoring system install plan for the Western Trawl Fisheries. [image: A white boat with many colored lights

AI-generated content may be incorrect.]
[image: A collage of different types of objects

AI-generated content may be incorrect.]

The e‑monitoring system must incorporate sensors to monitor gear activity and automatically trigger camera recording at the start and end of setting and hauling operations (also referred to as a “shot”), as well as during catch sorting. For Western Trawl Fishery vessels, the start of a shot (set) is when the otter boards have been deployed from the vessel, the end of the shot (haul) is when the boards are brought back onboard. 
To ensure adequate monitoring of catch sorting, the system must be configured with a run‑on recording time of 60 minutes following sensor activation.
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